1 AT Test UART Connection

2 AT+RESET Reset Device

3 AT+VERSION Querry ﬁrmware version

4 AT+ORGL Restore settings to Factory Defaults

5 AT+ADDR Query Device Bluetooth Address

6 AT+NAME Query/Set Device Name

7 AT+RNAME Query Remote Bluetooth Device’s Name

8 AT+ROLE Query/Set Device Role

9 AT+CLASS Query/Set Class of Device CoD

10 AT+IAC Query/Set Inquire Access Code

11 AT+INQM Query/Set Inquire Access Mode

12 AT+PSWD Query/Set Pairing Passkey

13 AT+UART Query/Set UART parameter

14 AT+CMODE Query/Set Connection Mode

15 AT+BIND Query/Set Binding Bluetooth Address

16 AT+POLAR Query/Set LED Output Polarity

17 AT+PIO Set/Reset a User I/O pin

18 AT+MPIO Set/Reset multiple User I/O pin

19 AT+MPIO? Query User I/O pin

20 AT+IPSCAN Query/Set Scanning Parameters

21 AT+SNIFF Query/Set SNIFF Energy Savings Parameters

22 AT+SENM Query/Set Security & Encryption Modes

23 AT+RMSAD Delete Authenticated Device from List

24 AT+FSAD Find Device from Authenticated Device List

25 AT+ADCN Query Total Number of Device from Authenticated Device List

26 AT+MRAD Query Most Recently Used Authenticated Device

27 AT+STATE Query Current Status of the Device

28 AT+INIT Initialize SPP Proﬁle

29 AT+INQ Query Nearby Discoverable Devices

30 AT+INQC Cancel Search for Discoverable Devices

31 AT+PAIR Device Pairing

32 AT+LINK Connect to a Remote Device

33 AT+DISC Disconnect from a Remote Device

34 AT+ENSNIFF Enter Energy Saving mode

35 AT+EXSNIFF Exit Energy Saving mode